#
STEERING TECHNICAL DATA

id065000800200

Item | Specification
--- | ---
Power steering fluid type | ATF M-III or equivalent (e.g. Dexron®II)
Power steering fluid capacity when reservoir tank is at maximum volume | 1.05 L {1.11 US qt, 0.92 Imp qt} (approximate quantity)
Oil pump fluid pressure (oil temperature 50-60 °C {122-140 °F}) | 9.31-9.80 MPa {95.0-99.9 kgf/cm2, 1360-1420 psi}
Gear housing fluid pressure (oil temperature 50-60 °C {122-140 °F}) | 9.31-9.80 MPa {95.0-99.9 kgf/cm2, 1360-1420 psi}
Steering wheel play | 0-30 mm {0-1.18 in} (When hydraulic operating)
Steering wheel effort | 7.8 N·m {80 kgf·cm, 69 in·lbf} or less (reference value)
Steering shaft length | 447 mm {17.6 in}
Steering rack runout | Large diameter portion: 0.15 mm {0.006 in} max. Small diameter portion: 0.20 mm {0.008 in} max.
Tie-rod end rotational torque | 0.42-2.60 N·m {4.29-26.5 kgf·cm, 3.72-23.0 in·lbf} [Pull scale reading: 4.2-26.0 N {0.43-2.65 kgf, 0.95-5.84 lbf}]
Tie rod swing torque | 0.1-4.6 N·m {2-46 kgf·cm, 1-40 in·lbf} [Pull scale reading: 0.6-29.3 N {0.06-2.98 kgf, 0.14-6.58 lbf}]