#
DRIVE BELT AUTO TENSIONER INSPECTION [ZJ, ZY]

id0110008017b7

1. Remove the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, ZY].)

2. Verify that the drive belt auto tensioner moves smoothly in the operational direction.

  • If it does not move smoothly, replace the drive belt auto tensioner.

3. Rotate the drive belt auto tensioner pulley by hand and verify that it rotates smoothly.

  • If it does not move smoothly, replace the drive belt auto tensioner.

4. Install the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, ZY].)