#
BONNET REMOVAL/INSTALLATION

id091000407200

  Warning

  • Removing the bonnet without proper support can be dangerous. The bonnet may fall and injure you. Always perform the following procedure with at least another person.

1. Disconnect the windshield washer hose.

2. To remove the bonnet hinge, remove the front fender panel.

3. Remove in the order indicated in the table.

1 | Bonnet insulator
2 | Shroud seal weatherstrip
3 | Bonnet
4 | Bonnet hinge
5 | Bonnet stay
6 | Bonnet lever
7 | Bonnet lock
8 | Bonnet release lever (See Bonnet Release Lever Removal Note)
9 | Bonnet release cable

4. Install in the reverse order of removal.

5. Adjust the bonnet. (See BONNET ADJUSTMENT.)

## Bonnet Release Lever Removal Note

1. Pull the lever.

2. While pushing the tab in the direction of the arrow using a tape-wrapped, small flathead screwdriver, disengage it from the dashboard.

  Caution

  • Remove the bonnet release lever while taking care not to damage the bonnet release cable with the flathead screwdriver.

3. Under the condition in Step 2, pull the bonnet release lever outward, then remove it from the dashboard.