#
PCM CONFIGURATION

id014000802600

1. Connect the WDS or equivalent to the DLC-2.

2. Set up the WDS or equivalent (including the vehicle recognition).

3. Select "Module Programming".

4. Select "Programmable Module Installation".

5. Select "PCM" and perform procedures according to directions on the WDS or equivalent screen.

  Note

  • If the PCM is replaced with a new one, the PCM stores DTC P0602 and illuminates the MIL even though no malfunction is detected. This means the PCM has not been configured yet.

6. Retrieve DTC's using the WDS or equivalent, then verify that there are no DTCs present.

  • If a DTC is present, perform the applicable DTC inspection.