#
REAR WIPER MOTOR INSPECTION

id091900475600

1. Disconnect the negative battery cable.

2. Remove the liftgate lower trim. (See LIFTGATE TRIM REMOVAL/INSTALLATION.)

3. Disconnect the rear wiper motor connector.

4. Connect battery positive voltage to the rear wiper motor terminal A, and ground the rear wiper motor terminal B to a bare metal part of the vehicle.

5. Verify that the rear wiper motor operates.

6. Disconnect the ground to the terminal B while the rear wiper is operating.

7. Verify that the rear wiper stops in the park position.

  • If there is any malfunction, replace the rear wiper motor.