#
VARIABLE VALVE TIMING ACTUATOR INSPECTION

id011000506000

  Caution

  • Variable valve timing actuator cannot be disassembled because it is a precision unit.

1. Verify that the camshaft knock pin hole of the rotor and the T-mark on the cover of the variable valve timing actuator are aligned and placed at the same position by rotating them by hand.

  Caution

  • If the camshaft knock pin hole and the T- mark are not aligned, rotate the rotor (the camshaft installing part) until a click is heard, and verify that they are fixed in place.

  • If the rotor is not secured even though their camshaft knock pin hole and the T-mark are aligned, replace the variable valve timing actuator.