#
PID/DATA MONITOR TABLE

id0802a0800800

PID name (Definition) | Unit/State | Detection state | SAS control module terminal
--- | --- | --- | ---
CCNT_RCM (Number of continuous DTCs) | - | • DTC is detected:1-255 • DTC is not detected:0 | -
D_CRSH_S (Driver-side side air bag sensor state) | OK/ COMM FAIL/ INT FAIL | • Sensor normal: OK • Sensor communication error: COMM FAIL • Sensor internal circuit abnormal: INT FAIL | 1S, 1R
D_PTENSFLT (Driver-side pre-tensioner seat belt circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1E, 1I
DS_AB_ST (Driver-side side air bag module circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1M, 1Q
DS_CURT_ST (Driver-side curtain air bag module circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1C, 1G
DSB_P_ST (Driver-side pre-tensioner seat belt circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1E, 1I
DS1_STAT (Driver-side air bag module (inflator No.1) circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 2J, 2N
DS2_STAT (Driver-side air bag module (inflator No.2) circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 2E, 2I
FNT_CRSH_S (Crash zone sensor state) | OK/ COMM FAIL/ INT FAIL | • Sensor normal: OK • Sensor communication error: COMM FAIL • Sensor internal circuit abnormal: INT FAIL | 1J, 1K
OD_D_CRSH (On demand driver-side side air bag sensor state) | OK/ COMM FAIL/ INT FAIL | • Sensor normal: OK • Sensor communication error: COMM FAIL • Sensor internal circuit abnormal: INT FAIL | 1R, 1S
OD_D_CURT (On demand driver-side curtain air bag module circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1C, 1G
OD_DAB1_ST (On demand driver-side air bag module (inflator No.1) circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 2J, 2N
OD_DAB2_ST (On demand driver-side air bag module (inflator No.2) circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 2E, 2I
OD_DSAB_ST (On demand driver-side side air bag module circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1M, 1Q
OD_P_CRSH (On demand passenger-side side air bag sensor state) | OK/ COMM FAIL/ INT FAIL | • Sensor normal: OK • Sensor communication error: COMM FAIL • Sensor internal circuit abnormal: INT FAIL | 1N, 1O
OD_P_CURT (On demand passenger-side curtain air bag module circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1D, 1H
OD_PSAB_ST (On demand passenger-side side air bag module circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1P, 1T
OD_F_CRSH (On demand crash zone sensor state) | OK/ COMM FAIL/ INT FAIL | • Sensor normal: OK • Sensor communication error: COMM FAIL • Sensor internal circuit abnormal: INT FAIL | 1J, 1K
OD_PAB1_ST (On demand passenger-side air bag module (inflator No.1) circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 2R, 2V
OD_PAB2_ST (On demand passenger-side air bag module (inflator No.2) circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 2M, 2Q
P_CRSH_S (Passenger-side side air bag sensor state) | OK/ COMM FAIL/ INT FAIL | • Sensor normal: OK • Sensor communication error: COMM FAIL • Sensor internal circuit abnormal: INT FAIL | 1N, 1O
P_PTESFLT (Passenger-side pre-tensioner seat belt circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1A, 1B
PS_AB_ST (Passenger-side side air bag module circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1P, 1T
PS_CURT_ST (Passenger-side curtain air bag module circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1D, 1H
PSB_P_ST (Passenger-side pre-tensioner seat belt circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 1A, 1B
PS1_STAT (Passenger-side air bag module (inflator No.1) circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 2R, 2V
PS2_STAT (Passenger-side air bag module (inflator No.2) circuit state) | SHRT GND/ SHRT B+/ OPEN/ SQ_LOWRES/ NORMAL | • Related wiring harness short to ground: SHRT GND • Related wiring harness short to power supply: SHRT B+ • Related wiring harness circuit open: OPEN • Pre-tensioner seat belt circuit resistance low: SQ_LOWRES • Related wiring harness normal: NORMAL | 2M, 2Q
VBATT (Battery voltage) | V | Under any condition: B+ | 2U