#
UNDERBODY FLAT-PLANE DIMENSIONS

id098010740400

.

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Front side frame standard hole | ø16 {0.63}
B | Front crossmember mounting bolt | ø17 {0.67}
C | Front suspension mounting block standard hole | ø31 {1.22}
D | Front frame rear standard hole | 16 × 25
{0.63 × 0.98}
E | Lower arm bracket standard hole | ø10 {0.39}
F | Front frame rear standard hole | ø16 {0.63}
G | Front frame rear standard hole | 18 × 38
{0.71 × 1.50}
H | Front B frame standard hole | 16 × 20
{0.63 × 0.79}
I | Rear side frame standard hole | ø16 {0.63}
J | Link bracket standard hole | ø12 {0.47}
K | suspension mounting block standard hole | ø16 {0.63}
L | Rear suspension housing bolt | ø6 {0.24}