#
INSTRUMENT CLUSTER SPECIFICATIONS

id092200101100

Item | Specification
--- | ---
Speedometer | Meter type | Stepping motor type
Indication range | (km/h) | 0-200
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Tachometer | Meter type | Stepping motor type
Indication range | (rpm) | 0-8,000
Red zone | (rpm) | 6,500-8,000
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Fuel gauge | Meter type | Stepping motor type (Reset-to-zero type)
Input signal communication system | Conventional communication system
Input signal source | Fuel gauge sender unit
Rated voltage | (V) | DC 12
Water temperature gauge | Meter type | Stepping motor type (Medium range stabilized type)
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Odometer/Tripmeter | Display | LCD
Indication digits | Odometer: 6 digits, Tripmeter: 4 digits
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12