#
HOLD SWITCH REMOVAL/INSTALLATION [FN4A-EL]

id0517a1291300

1. Disconnect the negative battery cable.

2. Remove the console.

3. Disconnect the connector and remove the HOLD switch terminals. (See SELECTOR LEVER DISASSEMBLY/ASSEMBLY.)

4. Remove the selector lever knob component.

5. Remove the HOLD switch.

6. Install the HOLD switch to selector lever knob component.

7. Install selector lever knob component.

Tightening torque

  2-3 N·m {21-30 kgf·cm, 19-26 in·lbf}

8. Connect the connector.

9. Install the console.

10. Connect the negative battery cable.