AUTOMATIC TRANSAXLE DISASSEMBLY

id051700502100

Precaution

General notes

  • The oil pan could contain small chips, shavings, and other particles which may be helpful in inspecting the condition of the transaxle and diagnosing certain problems.
  To ensure that all foreign particles stay in the oil pan, make sure that the transaxle is never tipped completely over while the oil pan is still installed.
    1. Disassemble the transaxle in a clean area (dustproof work space) to prevent entry of dust into the mechanisms.
    2. Inspect the individual transaxle components in accordance with the QUICK DIAGNOSIS CHART during disassembly.
    3. Use only plastic hammers when applying force to separate the light alloy case joints.
    4. Never use rags during disassembly; they may leave particles that can clog fluid passage.
    5. Several parts resemble one another; arrange them so that they do not get mixed up.
    6. Disassemble the control valve component and thoroughly clean it when the clutch or brake band has burned or when the ATF has degenerated.

  Warning
  • Although the stand has a self-locking brake system, there is a possibility that the brake may not hold when the transaxle is held in a lopsided position on the stand. This would cause the transaxle to turn suddenly, causing serious injury. Never keep the transaxle tilted to one side. Always hold the rotating handle firmly when turning the transaxle.

Disassembly

Components

baf4za00000137

1 | Torque converter
2 | Oil dipstick and oil filler tube
3 | Input/turbine speed sensor
4 | Oil pressure switch
5 | Transaxle range switch
6 | Vehicle speed sensor
7 | Connector pipe
8 | Connector bolt
9 | Oil pipe
10 | Oil pan
11 | Control valve body component
12 | Oil pump
13 | Thrust washer
14 | End cover
15 | Needle bearing

baf4za00000002

1 | 2–4 brake band
2 | Needle bearing
3 | Clutch component
4 | Snap ring
5 | Rear planetary gear component
6 | Needle bearing
7 | Front sun gear
8 | Needle bearing
9 | Front planetary gear component
10 | Front internal gear and one-way clutch
11 | Lock nut
12 | Bearing
13 | Distance piece
14 | Snap ring
15 | Low and reverse brake
16 | Snap ring
17 | One-way clutch inner race
18 | Piston return spring
19 | Low and reverse brake piston

baf4za00000003

1 | Manual shaft
2 | Servo apply accumulator
3 | Forward accumulator
4 | Parking rod lever component
5 | Band servo
6 | Differential
7 | Secondary gear and output gear
8 | Actuator plate
9 | Support actuator
10 | Parking pawl shaft
11 | Parking pawl
12 | Pawl return spring
13 | Forward clutch
14 | Forward clutch hub
15 | Primary gear
16 | Bearing race
17 | Funnel
18 | Oil pipe
19 | Oil seal
20 | Transaxle case

baf4za00000004

1 | Bearing race
2 | Adjustment shim
3 | Oil seal
4 | Converter housing

Disassembly procedure

1. Remove the torque converter, and immediately turn it so that the hole faces upward.

This will help to keep any remaining fluid from spilling.

2. Remove the ATF dipstick and oil filler tube.

3. Remove the O-ring from the oil filler tube.

4. Remove the breather hose.

5. Assemble the SST.

baf4za00000005

6. Lift the transaxle and mount it on the SST.

baf4za00000006

7. Remove the input/turbine speed sensor.

8. Remove the O-ring from the input/turbine speed sensor.

9. Remove the oil pressure switch. (with oil pressure switch)

10. Remove the transaxle range switch.

11. Remove the vehicle speed sensor.

12. Remove the O-ring from the vehicle speedometer sensor.

13. Remove the connector pipe, connector bolt and oil pipe.

  Warning
  • Using compressed air can cause dirt and other particles to fly, out, causing injury to the eyes. Wear protective eye wear whenever using compressed air.

  Caution
  • Clean the transaxle exterior thoroughly with a steam cleaner or cleaning solvents before removal.
  • If any old sealant gets into the transaxle during installation of the oil pan, trouble may occur in the transaxle. Remove any old sealant from the transaxle case and oil pan, and clean with cleaning fluids.

14. Remove the oil pan.

Examine any material found in the pan or on the magnet to determine the condition of the transaxle. If large amounts of material are found, replace the torque converter and carefully inspect the transaxle for the cause.

  (1) Clutch facing material
    • Drive plate and brake band wear

  (2) Steel (magnetic)
    • Bearing, gear, and driven plate wear

  (3) Aluminum (nonmagnetic)
    • Aluminum part wear

15. Disconnect the solenoid valve connector, ground, and transaxle fluid temperature sensor.

baf4za00000007

16. Remove the oil strainer.

17. Remove the O-ring from the oil strainer.

baf4za00000008

18. Remove the bolts as shown in the figure.

baf4za00000009

  Note
  • Remove the control valve body by removing the head of the manual valve from the port of the parking assist lever component.

19. Remove the control valve body.

baf4za00000010

20. Remove the coupler component.

baf4za00000011

21. Remove the accumulator component.

baf4za00000012

22. Remove the manual shaft.

  (1) Remove the roll pin using a pin punch.

  baf4za00000013

  (2) Remove the manual shaft.

  (3) Remove the O-ring from the manual shaft.

  baf4za00000014

23. Remove the parking rod lever component.

baf4za00000015

24. Remove the band servo component.

baf4za00000016

25. Remove the oil pump.

baf4za00000017

26. Remove the converter housing by tapping lightly with a plastic hammer.

baf4za00000018

27. Remove the forward clutch component.

baf4za00000019

28. Remove the differential.

baf4za00000020

29. Remove the secondary gear and output gear.

baf4za00000021

30. Remove the actuator plate.

baf4za00000022

31. Remove the support actuator.

baf4za00000023

32. Pull out the parking pawl shaft.

baf4za00000024

33. Remove the parking pawl.

34. Remove the pawl return spring.

baf4za00000025

35. Remove the end cover.

36. Remove the O-ring from the transaxle case.

baf4za00000026

37. Remove the band strut.

baf4za00000027

38. Remove the 2–4 brake band, and hold it together using a piece of wire as shown in the figure.

baf4za00000028

39. Remove the clutch component.

baf4za00000029

40. Remove the snap ring.

baf4za00000030

41. Remove the rear planetary gear component.

baf4za00000031

42. Remove the front sun gear by tapping its end with a flathead screwdriver or similar tool. as shown in the figure.

baf4za00000032

43. Remove the forward clutch hub.

44. Remove the front planetary gear component.

baf4za00000033

45. Remove the front internal gear and one-way clutch component.

baf4za00000034

46. Remove the locknut.

  (1) Knock the crimped portion of the locknut outward by using a small chisel and a hammer.

  baf4za00000035

  (2) Install the SST to the primary gear in the order shown.

  baf4za00000036

    Tightening torque
    19—25 N·m {1.9—2.6 kgf·m, 14—18 ft·lbf}

  (3) Install the SST to the locknut in the order shown.

  baf4za00000037

  (4) Remove the locknut.

  baf4za00000038

47. Remove the primary gear by tapping it with a flathead screwdriver, etc. as shown in the figure.

baf4za00000039

48. Remove the bearing and distance piece.

baf4za00000040

  Caution
  • Removing the bearing race using a flathead screwdriver can damage the inside of the bearing race. Handle the flathead screwdriver carefully.

49. Remove torx screws from the converter housing side.

baf4za00000041

50. Remove the bearing race.

51. Remove the bearing race using the SST as shown in the figure.

baf4za00000042

52. Tap the funnel at the areas indicated in the figure using a flathead screwdriver, etc. to make gaps big enough to install the SST. Then remove the bearing race.

baf4za00000043

53. Remove the funnel.

  Caution
  • Removing the oil pipe using a flathead screwdriver can damage the oil pipe.
  Handle the flathead screwdriver carefully.

54. Remove the oil pipe.

baf4za00000044