#
AUDIO CONTROL SWITCH REMOVAL/INSTALLATION

id092000800200

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Remove the steering wheel. (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Screw
2 | Cover (See Cover Installation Note)
3 | Screw
4 | Audio control switch (See Audio Control Switch Installation Note)

5. Install in the reverse order of removal.

## Audio Control Switch Installation Note

1. Pass the audio control switch wiring harness under the horn bracket.

## Cover Installation Note

1. Fix the audio control switch wiring harness in the cover clip.