#
CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION

CDA014018230W02

  Caution

  • When replacing the CKP sensor, make sure there is no foreign material on it such as metal shavings. If it is installed with foreign material, the sensor output signal will malfunction resulting from fluctuation in magnetic flux and cause a deterioration in engine control.

1. Disconnect the negative battery cable.

2. Remove the splash shield.

3. Disconnect the CKP sensor connector.

4. Remove the CKP sensor installation bolts.

5. Remove the CKP sensor.

6. Install in the reverse order of removal.

Tightening torque

  7.8-10.8 N·m {0.8-1.1 kgf·m, 5.8-7.9 ft·lbf}