#
WHEEL APRON PANEL ASSEMBLY REMOVAL

id098008614900

## LH

1. Drill the 12 weld locations indicated by (A), and 3 weld locations indicated by (B), remove the wheel apron panel assembly.

  Note

  • If removing the wheel apron panel front and the suspension housing separately as separate parts, drill 3 locations indicated by (B) and drill 7 locations indicated by (C).

## RH

1. Remove the bolt from location (A).

2. Drill the 12 weld locations indicated by (B) and 5 weld locations indicated by (C), then remove the wheel apron panel assembly.

  Note

  • If removing the wheel apron panel front and the suspension housing separately as separate parts, drill 5 locations indicated by (C) and drill 7 locations indicated by (D).