#
AFTER REPAIR PROCEDURE [FN4A-EL]

id0502a1800400

  Caution

  • After repairing a malfunction, perform this procedure to verify that the malfunction has been corrected.
  • When this procedure is carried out, be sure to drive the vehicle at lawful speed and pay attention to the other vehicles.

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the ignition switch to the ON position (Engine OFF).

3. Verify that DTCs are cleared from memory.

4. Decrease ATF temperature to 20 °C {68 °F} or below.

5. Start the engine then wait 180 s or more.

6. Warm up the engine and ATX.

  • Engine coolant temperature: 60 °C {140 °F} or above.
  • Transaxle fluid temperature: 20 °C {68 °F} or above.

7. Shift the selector lever between P position to L range while depressing brake pedal.

8. Drive the vehicle for 150 s or more at a vehicle speed between 25 and 59 km/h {15 and 36 mph}, then 60 km/h {37 mph} or more for 100 s or more.

9. Drive the vehicle in D range and shift gears between 1st and 4th (TCC operation) gear.

10. Gradually slow down and stop the vehicle.

11. Make sure that the repaired DTC does not recur.