#
CYLINDER HEAD (II) DISASSEMBLY [WITHOUT DIESEL PARTICULATE FILTER]

id0110f4500500

1. Disassemble in the order indicated in the table.

1 | Glow plug, glow plug lead (See Glow Plug, Glow Plug Lead Disassembly Note)
2 | Engine coolant temperature sensor
3 | Cylinder head (See Cylinder Head Disassembly Note)
4 | Cylinder head gasket
5 | Valve keeper (See Valve Keeper Disassembly Note)
6 | Upper valve spring seat
7 | Valve spring
8 | Lower valve spring seat
9 | Valve
10 | Valve seal (See Valve Seal Disassembly Note)

## Glow Plug, Glow Plug Lead Disassembly Note

  Caution

  • Damaging heat-generating part of the plug can cause the plug to blow out. Do not use the plug if it is dropped from a height over 10 cm {3.9 in}.
  • When removing the glow plug, loosen it one or more threads using tool, then further loosen by hand and remove it.

## Cylinder Head Disassembly Note

• Loosen the cylinder head bolts in two or three steps in the order shown.

## Valve Keeper Disassembly Note

• Remove the valve keeper using the SSTs.

## Valve Seal Disassembly Note

1. Remove the valve seal using the SST.