#
EXHAUST GAS PRESSURE CORRECTION TEMPERATURE SENSOR CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1223600
• Installed to the dash lower panel in the engine compartment together with the exhaust gas pressure sensor.

.

1 | Exhaust gas pressure correction temperature sensor
2 | Exhaust gas pressure sensor

• The thermistor type exhaust gas pressure correction temperature sensor changes resistance according to the exhaust gas pressure sensor ambient temperature.

1 | Exhaust gas pressure correction temperature sensor
2 | Thermistor

• The resistance decreases if the exhaust gas pressure sensor ambient temperature increases and conversely increases if the exhaust gas pressure sensor ambient temperature decreases.

.

1 | Exhaust gas pressure correction temperature sensor
2 | Exhaust gas pressure correction temperature sensor characteristic
3 | Exhaust gas pressure sensor ambient temperature
4 | Resistance
5 | Large
6 | Small
7 | High
8 | Low