#
REAR LATERAL LINK REMOVAL/INSTALLATION

id021400801200

1. Remove the rear lateral link.

  Caution

  • When working near left rear suspension, avoid any impact to the fuel tank.

2. Measure the length L shown in the figure for proper installation.

3. Temporarily loosen a locknut of the rear lateral link.

4. Install the rear lateral link.

5. Inspect the rear wheel alignment.

(See REAR WHEEL ALIGNMENT.)