#
AUTO WIPER SYSTEM OPERATION

id091900101300

1. The rain sensor installed in the windshield detects rainfall amount when the wiper and washer switch is moved to the AUTO position.

2. The detected rainfall amount is converted to an electric signal and transmitted to the auto wiper control module as a windshield wiper operation control signal.

3. When the microcomputer in the auto wiper control module receives the control signal, the wiper relay turns on.

4. When the windshield wiper relay is on, current flows to the windshield wiper motor for wiper operation at low speed.

.

1 | Windshield wiper and washer switch
2 | Windshield washer switch
3 | Auto wiper control module
4 | Microcomputer
5 | Windshield wiper motor
6 | Windshield washer motor
7 | Rain sensor

## Interval Operation

• If the windshield wipers are stopped and the rain sensor detects a specified amount of rainfall, the wipers are operated at low speed. The interval timing is adjusted according to the amount of rainfall detected.

### Low speed operation

  • If the windshield wipers are operating at intervals and the rain sensor detects a specific amount of rainfall, the wipers are operated continuously at low speed.

### High speed operation

  • If the windshield wipers are operating at low speed or stopped and the rain sensor detects an amount of rainfall that is greater than that for low speed operation, the wipers are operated two times at high speed. After operating at high speed two times, if the rain sensor detects an amount of rainfall that is greater than that for low speed operation, the wipers continue to operate at high speed.