#
BRAKE SIGNAL CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1224400
• While the brake pedal is depressed, the brake switch No.1 contact point closes (ON) and the PCM detects B+. While the brake pedal is released, the brake switch No.1 contact point opens (OFF) and the PCM detects below 1.0 V.
• While the brake pedal is depressed, the brake switch No.2 contact point opens (OFF) and the PCM detects B+. While the brake pedal is released, the brake switch No.2 contact point closes (ON) and the PCM detects below 1.0 V.

1 | Brake switch No.1
2 | Brake light
3 | Switch ON
4 | Switch OFF
5 | Brake pedal depressed
6 | Brake pedal released
7 | Brake switch No.2