#
INPUT/TURBINE SPEED SENSOR INSPECTION [JA5AX-EL]

id051705801200

## On-Vehicle Inspection

1. Disconnect the terminal component No.2 connector.

2. Measure resistance between the terminals E and F.

  • If not as specified, inspect the input/turbine speed sensor. (See Inspection of Individual Part.)

Input/turbine speed sensor

  Resistance: 513-627 ohms (ATF temperature: 20 °C {68 °F})

3. Connect the terminal component No.2 connector.

## Inspection of Individual Part

1. Remove the input/turbine speed sensor. (See INPUT/TURBINE SPEED SENSOR REMOVAL/INSTALLATION [JA5AX-EL].)

2. Measure resistance between the terminals of the input/turbine speed sensor.

  • If not as specified, replace the input/turbine speed sensor.
  • If it is normal, replace the harness.

Input/turbine speed sensor

  Resistance: 513-627 ohms (ATF temperature: 20 °C {68 °F})

3. Install the input/turbine sensor. (See INPUT/TURBINE SPEED SENSOR REMOVAL/INSTALLATION [JA5AX-EL].)