#
INTERIOR LIGHT CONTROL SYSTEM OPERATION

id091800526000

Conditions before operation (Conditions which must be satisfied) | Operation condition | Interior light | Cancel condition (When any condition satisfied)
--- | --- | --- | ---
Illumination time | Brightness
• Turn the ignition switch to the LOCK or ACC position. • All doors are closed. (All door switches off) | Any door open. (Any door switch on) | Approx.30 min | 100 % | • All doors are closed except liftgate. (All door switches off) • After illumination time.*1
• Key extracted from steering lock. (Key reminder switch is off.) • All doors are closed. (All ddoor switches off) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) | Driver's door lock knob is unlocked. (Door lock-link switch is in unlock position.) | Approx.30 s | 100 % | • Turn the ignition switch to the ON position. • Any door open. (Any door switch on) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*1
• Key inserted into steering lock. (Key reminder switch is on.) • All doors are closed. (All door switches off) | Key extracted from steering lock. (Key reminder switch is off.) | Approx.15 s | 100 % | • Turn the ignition switch to the ON position. • Any door open. (Any door switch on) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*1
• Turn the ignition switch to the LOCK or ACC position. • Any door is open. (Any door switches on) • Driver's door lock knob is unlocked. (Door lock-link switch is in unlock position.) | All doors are closed. (All door switches off) | Approx.15 s | 60 % | • Turn the ignition switch to the ON position. • Any door open. (Any door switch on) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*1

  *1 :
After interior light is turned off according to this cancel condition, the light will illuminate again when either of the following conditions are satisfied:
• After all doors are closed, then any door is reopened.
(After all door switches are off, any door switch is on)
• After all doors are closed, then ignition switch is at the ON position. (IG ON)

.

1 | Door lock-link switch
2 | Door
3 | Key reminder switch
4 | Front map light/rear map light/courtesy light/ignition key illumination
5 | Lock
6 | Unlock
7 | CLOSE
8 | OPEN
9 | ON
10 | OFF
11 | 100%
12 | 60%
13 | 0%
14 | View A
15 | Approx. 30 s
16 | Approx. 15 s
17 | Approx. 1 s
18 | Approx. 30min