#
HEADLINER REMOVAL/INSTALLATION [WGN]

id0917004583a2

1. Disconnect the negative battery cable.

2. Turn the seaming welt and weatherstrip over.

3. Remove the sunroof seaming welt. (vehicles with sunroof only)

4. Remove the A-pillar trims.

5. Remove the B-pillar upper trims.

6. Remove the C-pillar trims.

7. Remove the D-pillar trims.

8. Remove the front and rear map light.

9. Remove the cargo compartment light. (See CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION [WGN].)

10. Remove the sunvisors.

11. Remove the assist handle.

12. Remove the net anchor.

13. Disconnect the roof harness connector, remove the clip, and remove the connector.

14. Disconnect the front and rear drain hose.

15. Disconnect the rear washer hose.

16. Place the rear center seat belt bezel out of the way of the headliner.

17. Remove the fasteners.

18. Remove the hook holding the roof panel and remove the headliner.

19. Take the headliner off from the liftgate opening.

20. Install in the reverse order of removal.