#
BRAKES TECHNICAL DATA

id045000800100

Item | Specification
--- | ---
Brake fluid type | European (L.H.D. U.K.) specs.: SAE J1703, FMVSS 116 DOT-3 or DOT-4 Australian, General (L.H.D. R.H.D.) specs.: SAE J1703, FMVSS 116 DOT-3
Brake pedal height (reference value) | L.H.D.: 187 mm {7.36 in} R.H.D.: 172 mm {6.77 in}
Brake pedal play | 0-3 mm {0-0.1 in}
Brake pedal-to-floor clearance (Brake pedal when depressed at 588 N {60 kgf, 132 lbf}) | 68 mm {2.7 in} or more
Power brake unit fluid pressure when pedal depressed at 200 N {20 kgf, 44 lbf} | At 0 kPa {0 mmHg, 0 inHg}: 590 kPa {6.02 kgf/cm2, 85.6 psi}
Power brake unit fluid pressure when pedal depressed at 200 N {20 kgf, 44 lbf} | At 66.7 kPa {500 mmHg, 19.7 inHg}: 8,780 kPa {89.53 kgf/cm2, 1,273 psi}
Proportioning valve fluid pressure (without ABS (ABS/TCS) or DSC) | Rear brake fluid pressure when front brake fluid pressure at 2,450 kPa {25 kgf/cm2, 355 psi}: 2,450 kPa {25 kgf/cm2, 355 psi} ± 200 kPa {2 kgf/cm2, 29 psi} Rear brake fluid pressure when front brake fluid pressure at 5,880 kPa {60 kgf/cm2, 853 psi}: 3,480 kPa {35.5 kgf/cm2, 505 psi} ± 300 kPa {3 kgf/cm2, 44 psi}
Front disc plate runout limit | 0.05 mm {0.002 in}
Minimum front disc plate thickness (European (L.H.D. U.K.) specs.) | L8 (4SDN, 5HB): 22 mm {0.87 in} L8 (WGN), LF, L3, L3 Turbo, MZR-CD (RF Turbo): 23 mm {0.91 in}
Minimum front disc plate thickness (Australian, General (L.H.D. R.H.D.) specs.) | 4SD (except L3 Turbo), 5HB, WGN (except Australian specs.): 22 mm {0.87 in} 4SD (L3 Turbo), WGN (Australian specs.): 23 mm {0.91 in}
Minimum front disc plate thickness after machining using a brake lathe on-vehicle (European (L.H.D. U.K.) specs.) | L8 (4SDN, 5HB): 22.8 mm {0.90 in} L8 (WGN), LF, L3, L3 Turbo, MZR-CD (RF Turbo): 23.8 mm {0.94 in}
Minimum front disc plate thickness after machining using a brake lathe on-vehicle (Australian, General (L.H.D. R.H.D.) specs.) | 4SD (except L3 Turbo), 5HB, WGN (except Australian specs.): 22.8 mm {0.90 in} 4SD (L3 Turbo), WGN (Australian specs.): 23.8 mm {0.94 in}
Minimum front disc pad thickness (European (L.H.D. U.K.) specs.) | L8 (4SDN, 5HB): 2.0 mm {0.079 in} min. L8 (WGN), LF, L3, L3 Turbo, MZR-CD (RF Turbo): 1.5 mm {0.059 in} min.
Minimum front disc pad thickness (Australian, General (L.H.D. R.H.D.) specs.) | 4SD (except L3 Turbo), 5HB, WGN (except Australian specs.): 2.0 mm {0.079 in} min. 4SD (L3 Turbo), WGN (Australian specs.): 1.5 mm {0.059 in} min.
Rear disc plate runout limit | 0.05 mm {0.002 in}
Minimum rear disc plate thickness | Except 18 inch wheel: 8 mm {0.31 in} 18 inch wheel: 9 mm {0.35 in}
Minimum rear disc plate thickness after machining using a brake lathe on-vehicle | Except 18 inch wheel: 8.8 mm {0.35 in} 18 inch wheel: 9.8 mm {0.39 in}
Minimum rear disc pad thickness | 2.0 mm {0.079 in} min.
Parking brake lever stroke when pulled at 98 N {10 kgf, 22 lbf} | 2-5 notches