#
STABILIZER CONTROL LINK INSPECTION

id021400803900

1. Remove the stabilizer control link from the vehicle.

2. Inspect for bending and damage.

3. Measure the ball joint starting torque.

  (1) Rock the ball joint stud side to side 10 times.
  (2) Rotate the ball joint stud 10 times.
  (3) Measure the starting torque using a suitable Allen socket and a torque wrench.
Rear stabilizer control link starting torque

  0.23-0.47 N·m {2.4-4.7 kgf·cm, 2.1-4.1 in·lbf}