#
DTC B2619

id0902i7856800

DTC B2619 | Rear auto leveling sensor signal system.
--- | ---
DETECTION CONDITION | Warning • incorrect servicing of the auto leveling control module could result in electrical shock because the unit is integrated with the discharge headlight control module. Before servicing the auto leveling control module, always refer to "Discharge headlight service warnings." (See DISCHARGE HEADLIGHT SERVICE WARNINGS) Output signal is not sent from the rear auto leveling sensor.
POSSIBLE CAUSE | • Rear auto leveling sensor malfunction • Open or short circuit in wiring harness between rear auto leveling sensor and headlight (LH) • Headlight (LH) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT REAR LEVELING SENSOR CONNECTION • Check installation condition of rear auto leveling sensor and fit of connector. • Are installation condition and fit okay? | Yes | Go to next step.
No | After correcting fit, clear DTC and check DTC again. • If DTC is displayed again, go to next step.
2 | INSPECT WIRING HARNESS BETWEEN REAR AUTO LEVELING SENSOR CONNECTOR AND HEADLIGHT (LH) CONNECTOR • Disconnect rear auto leveling sensor connector (6-pin) and headlight (LH) connector (4-pin). • Is there continuity between the following connectors? - Rear auto leveling sensor connector (terminal B) and headlight (LH) connector (terminal 2D) | Yes | Go to next step.
No | Repair or replace wiring harness between rear auto leveling sensor and headlight (LH).
3 | INSPECT WIRING HARNESS BETWEEN REAR AUTO LEVELING SENSOR CONNECTOR AND HEADLIGHT (LH) CONNECTOR • Disconnect rear auto leveling sensor connector (6-pin) and headlight (LH) connector (4-pin). • Is there no continuity between the following connectors? - Rear auto leveling sensor connector (terminal B) and headlight (LH) connector (terminal 2B) - Rear auto leveling sensor connector (terminal B) and headlight (LH) connector (terminal 2A) | Yes | Go to next step.
No | Repair or replace wiring harness between rear auto leveling sensor and headlight (LH).
4 | INSPECT HEADLIGHT (LH) • Disconnect auto leveling control module (main) connector (20-pin) and headlight (LH) connector (4-pin). • Is there continuity between the following connectors? - Auto leveling control module (main) connector (terminal F) and headlight (LH) connector (terminal 2D) | Yes | Go to next step.
No | Possible cause is an open circuit in headlight (LH). Replace headlight (LH). (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION)
5 | INSPECT HEADLIGHT (LH) • Disconnect auto leveling control module (main) connector (20-pin) and headlight (LH) connector (4-pin). • Is there no continuity between the following connectors? - Auto leveling control module (main) connector (terminal G) and headlight (LH) connector (terminal 2D) - Auto leveling control module (main) connector (terminal K) and headlight (LH) connector (terminal 2D) - Auto leveling control module (main) connector (terminal E) and headlight (LH) connector (terminal 2D) | Yes | Replace rear auto leveling sensor. (See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION [2WD]) (See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION [4WD])
No | Possible cause is an open circuit in headlight (LH). Replace headlight (LH). (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION)