#
SECURITY LIGHT: DTC 12 (WDS OR EQUIVALENT: DTC B2103)

id0902e5914600

DTC B2103 | Coil antenna not connected.
--- | ---
POSSIBLE CAUSE | • Defective coil antenna • Poor connection of coil antenna connector

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
- | INSPECT CONNECTOR CONNECTION • Is connector of coil antenna and PCM connected securely? | Yes | Replace coil antenna. (See COIL ANTENNA REMOVAL/INSTALLATION [KEYLESS ENTRY SYSTEM])
No | Connect connector securely.