#
MANUAL MODE SHIFT CONTROL OUTLINE [JA5AX-EL]

id051705102700

## Features

• The manual mode shift control is activated by moving the selector lever from the D to M range position (selector lever is shifted over toward front passenger side).
• Manual mode shift control with a manual shifting system allowing selection of gear positions by manual operation of the selector lever forward (-) and back (+) has been adopted. Moreover, engine braking for all gears in manual mode according to the gear ratio is available.

  - Shifting between 1GR and 2GR when the vehicle is stopped is possible.
  - When shifting from the D to M range while driving, the same gear position is maintained.
  - Consecutive shifting in the M range has been adopted. When shifting down from M range 4GR or 3GR, one gear can be skipped over by rapidly tapping the selector lever two times in the down-shift (-) direction.

• Selector lever position and gear position indicator lights, built into the instrument cluster, have been adopted.

  - The selector indicator light includes a selector lever position indicator that displays selector lever positions and, a gear position indicator light that displays gear positions.

## Construction (System Diagram)

.

1 | PCM
2 | TCM
3 | Output
4 | Ignition timing signal
5 | Line pressure control signal
6 | Clutch pressure control signal
7 | Engine
8 | ATX
9 | Indication
10 | Selector indicator light
11 | Gear position indicator light
12 | AT warning light
13 | Instrument cluster
14 | Input
15 | Selector lever component
-M range switch
-Up switch
-Down switch
16 | TR switch
17 | ABS HU/CM or DSC HU/CM
18 | TFT sensor