#
CLUTCH PEDAL POSITION (CPP) SWITCH INSPECTION [L3 Turbo]

id0140b6801600

  Note

  • Perform the following inspection only when directed.

## Continuity Inspection

1. Verify that the clutch switch is installed properly.

2. Disconnect the negative battery cable.

3. Remove the clutch switch. (See CLUTCH PEDAL REMOVAL/INSTALLATION.)

4. Inspect for continuity between the clutch switch terminals using a tester.

  • If the clutch switch is normal, but PID value is out of specification, perform the "Circuit Open/Short Inspection".
  • If not as specified, replace the clutch switch.

Specification

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [L3 Turbo].)

2. Inspect the following harnesses for an open or short circuit. (Continuity check)

### Open circuit

  • If there is no continuity, there is an open circuit. Repair or replace the wiring harness.
  - Clutch switch terminal A and PCM terminal 1H
  - Clutch switch terminal B and body ground

### Short circuit

  • If there is continuity, there is a short circuit. Repair or replace the wiring harness.
  - Clutch switch terminal B and power supply
  - Clutch switch terminal B and body ground