#
INSPECTION AFTER TRANSAXLE INSTALLATION [G66M-R]

id0515k1800300

  Note

  • Perform the following inspection only when the transaxle has been overhauled.

1. Perform a road test and inspect the following items:

  (1) No abnormal noise in each shift position.
  (2) Smooth shift operation when shifting gears.
  (3) No gear slipout after shifting gears.
  (4) Back-up light switch operates correctly.