#
BATTERY REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo]

id0117b1800500

1. Remove in the order indicated in the table.

1 | Negative battery cable
2 | Positive battery cable
3 | Battery clamp
4 | Battery box (See Battery Box Installation Note.)
5 | Battery
6 | Battery tray

2. Install in the reverse order of removal.

## Battery Box Installation Note

1. Install the battery box so that the side with the larger notch faces toward the front fender (LH).