#
REAR MAP LIGHT REMOVAL/INSTALLATION

id091800810500

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Rear map light (See Rear Map Light Removal Note.)
2 | Connector
3 | Socket
4 | Rear map light bulb

3. Install in the reverse order of removal.

## Rear Map Light Removal Note

1. Insert a tape-wrapped flathead screwdriver into the gap between the headliner and the rear map light.

2. Push the hooks to remove the rear map light.