#
EVAPORATOR INSPECTION

id071100801500

1. Remove the A/C unit. (See A/C UNIT REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo].) (See A/C UNIT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Remove the evaporator from the A/C unit.

3. Inspect for cracks, damage, and oil leakage.

  • If any problems are found, replace the evaporator.

4. Inspect for bent fins.

  • If any are bent, use a flathead screwdriver to straighten them.