#
DIFFERENTIAL ASSEMBLY

D6E051527100103

  Caution

  • Do not place the bearing (ring gear side) facing downward on a workbench after assembling the differential component. It may cause damage to the bearing roller guide.

1. Assemble in the order shown in the figure.

1 | Gear case component
2 | Ring gear (See Ring Gear Assembly Note.)
3 | Bearing (ring gear-opposite side) (See Bearing (Ring Gear-Opposite Side) Assembly Note (Except L3 Turbo).) (See Bearing (Ring Gear-Opposite Side) Assembly Note (L3 Turbo).)
4 | Bearing (ring gear side) (See Bearing (Ring Gear Side) Assembly Note.)

## Ring Gear Assembly Note

1. Assemble the gear case component and ring gear, and tighten the bolts in a criss-cross pattern in a few passes.

  Tightening torque
  99.7-112.3 N·m
  {10.2-11.4 kgf·m, 73.6-82.8 ft·lbf}

## Bearing (Ring Gear-Opposite Side) Assembly Note (Except L3 Turbo)

1. Install a new bearing using the SSTs and press.

## Bearing (Ring Gear-Opposite Side) Assembly Note (L3 Turbo)

1. Install a new bearing using the SSTs and press.

## Bearing (Ring Gear Side) Assembly Note

1. Install a new bearing using the SSTs and press.