#
TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR CONSTRUCTION/OPERATION [FS5A-EL]

id051721109000
• The TFT sensor is a thermistor type and the resistance changes according to the ATF temperature.
• The characteristic of the resistance is as shown in the figure below: when the ATF temperature increases, the resistance decreases, and when the ATF temperature decreases, the resistance increases.

1 | Oil strainer
2 | TFT sensor

1 | Resistance
2 | ATF temperature
3 | Characteristic of TFT sensor
4 | Increases