#
CLIMATE CONTROL UNIT WIRE ADJUSTMENT

id074000802100

## Air Mix Wire

1. Set the temperature control dial at max cold.

2. Set the air mix link to max cold in the direction shown by the arrow and insert a screwdriver at the set hole.

3. Connect the air mix wire to air mix link.

4. Clamp the air mix wire to wire clamp.

5. Verify that the temperature control dial moves its full stroke.

## Airflow Mode Wire

1. Set the airflow mode control dial at defroster.

2. Set the airflow mode main link to defroster in the direction shown by the arrow and insert a screwdriver at the set hole.

3. Connect the airflow mode wire to airflow mode main link.

4. Clamp the airflow mode wire to wire clamp.

5. Verify that the airflow mode control dial moves its full stroke.