#
FRONT FOG LIGHT AIMING

id091800468700

## Type A

1. Adjust the tire air pressure to the specification.

2. Position the unloaded vehicle on a flat, level surface.

3. Seat one person in the driver's seat.

4. Position the vehicle 3 m {10 ft} in front of a white screen.

5. While adjusting one fog light, mask the other.

6. Start the engine to charge the battery.

7. Turn the front fog light on.

8. Adjust the front fog light as shown in the figure.

## Type B

1. Adjust the tire air pressure to the specification.

2. Position the unloaded vehicle on a flat, level surface.

3. Seat one person in the driver's seat.

4. Position the vehicle 3 m {10 ft} in front of a white screen.

5. While adjusting one fog light, mask the other.

6. Start the engine to charge the battery.

7. Turn the front fog light on.

8. Slightly bend back the mudguard.

9. Adjust the front fog light as shown in the figure.