#
AUTOMATIC TRANSAXLE BASIC INSPECTION [JA5AX-EL]

id050305800300

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn ignition switch to ON. • Does gear position indicator light (illuminate/go out) corresponding to selector lever position? | Yes | Go to next step.
No | Perform symptom troubleshooting No.27 "Gear position indicator light does not illuminate in M range" No.28 "Gear position indicator light illuminates in D range or P, N, R positions".
2 | • Turn ignition switch to ON. • When selector lever is moved, are selector lever position and indicator aligned? Also, when other ranges are selected from N or P during idling, does vehicle creep within 1- 2 s? | Yes | Go to next step.
No | Inspect selector lever. (See SELECTOR LEVER INSPECTION.) Repair or replace defected areas.
3 | • Inspect ATF color and condition. (See Automatic Transaxle Fluid (ATF) Condition Inspection.) • Are ATF color and odor normal? | Yes | Go to next step.
No | Repair or replace any defective parts according to inspection result. Flush ATX and cooler line as necessary.
4 | • Perform line pressure test. (See Line Pressure Test.) • Is line pressure okay? | Yes | Go to next step.
No | Adjust accelerator cable as necessary. Repair or replace any defective parts according to inspection result.
5 | • Perform stall test. (SeeStall Speed Test.) • Is stall speed okay? | Yes | Go to next step.
No | Repair or replace any defective parts according to inspection result.
6 | • Inspect value at following PIDs using WDS or equivalent. (See TCM INSPECTION [JA5AX-EL].) - TFT - VPWR_TCM - TRD - RPM - TRR - THOP - CPP/PNP - TSS - VSS - OSS - MNL_SW - DWN_SW - UP_SW • Are PID values okay? | Yes | Perform symptom troubleshooting and follow procedures.
No | Repair or replace any defective parts according to inspection result.