#
INTAKE AIR TEMPERATURE (IAT) SENSOR NO.2 CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1181600
• Installed on the charge air cooler.
• The thermistor type IAT sensor No.2 changes resistance changes according to the IAT.
• The resistance decreases if the IAT increases and, conversely, increases if the IAT decreases.

1 | Thermistor
2 | IAT sensor No.2
3 | IAT sensor No.2 characteristic
4 | Resistance
5 | Large
6 | Small
7 | High
8 | Low