#
REMOTE CONTROLLER CONSTRUCTION/OPERATION

id092000104800
• When the remote controller is operated, infrared light is output from the transmitter on the end of the remote controller. The operation signal is sent to the center panel module using the infrared light.

.

No. | Button | Function
--- | --- | ---
1 | MUTE button | Mute
2 | POWER button | Power ON/OFF
3 | MODE button | Audio mode changes (FM1→FM2→AM→CD→HDD→AUX*)
4 | MENU button | Menu screen is displayed
5 | DISP button | Playback display changes
6 | ALL button | HDD playback mode changes to all tracks playback mode
7 | CATEGORY button | HDD playback mode changes to selected category playback mode
8 | ARTIST button | HDD playback mode changes to selected artist playback mode
9 | FAVORITE button | HDD playback mode changes to favorite track playback mode
10 | TRK/SEEK UP button | Lightly press (less than 1.5 s) | • Track up during CD or HDD playback • Cursor moves to the right during track information input
Press and hold (1.5 s or more) | • Track fast-forward during CD or HDD playback • Seek up during radio mode
11 | TRK/SEEK DOWN button | Lightly press (less than 1.5 s) | • Track down during CD or HDD playback • Cursor moves to the left during track information input
Press and hold (1.5 s or more) | • Track reverse during CD or HDD playback • Seek down during radio mode
12 | DISC UP button | Album change (UP) during HDD playback
13 | DISC DOWN button | Album change (DOWN) during HDD playback
14 | ENT. button | Enter key
15 | Number and symbol keys | Number, character, and symbol input
16 | CANCEL button | Lightly press (less than 1.5 s) | • Selected item or mode is canceled • Delete one character during character input
Press and hold (1.5 s or more) | Delete all characters during character input
17 | SCAN button | Scan play
18 | RPT button | Repeat play
19 | RDM button | Random play
20 | VOL button (-) | Volume down
21 | VOL button (+) | Volume up

  * :
Vehicles with TV tuner or auxiliary unit only