#
DTC TABLE [L8, LF, L3]

id0102a1545200
×: Applicable
-: Not applicable

DTC No. | Condition | MIL | DC | Monitor item | Self-test type*1 | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0011 | CMP timing over-advanced | ON | 1 | CCM | C, R | × | (See DTC P0011 [L8, LF, L3].)
P0012 | CMP timing over-retarded | ON | 2 | CCM | C, R | × | (See DTC P0012 [L8, LF, L3].)
P0030 | A/F sensor heater control circuit problem | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (SeeDTC P0030 [L8, LF, L3].)
P0031 | A/F sensor heater circuit low input | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0031 [L8, LF, L3].)
P0032 | A/F sensor heater circuit high input | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0032 [L8, LF, L3].)
P0037 | HO2S heater circuit low input | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0037 [L8, LF, L3].)
P0038 | HO2S heater circuit high input | ON | 2 | A/F sensor heater, HO2S heater | C, O, R | × | (See DTC P0038 [L8, LF, L3].)
P0101 | MAF sensor circuit range/performance problem | ON | 2 | CCM | C | × | (See DTC P0101 [L8, LF, L3].)
P0102 | MAF sensor circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0102 [L8, LF, L3].)
P0103 | MAF sensor circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0103 [L8, LF, L3].)
P0107 | MAP sensor circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0107 [L8, LF, L3].)
P0108 | MAP sensor circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0108 [L8, LF, L3].)
P0111 | IAT sensor circuit range/performance problem | ON | 2 | CCM | C | × | (See DTC P0111 [L8, LF, L3].)
P0112 | IAT sensor circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0112 [L8, LF, L3].)
P0113 | IAT sensor circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0113 [L8, LF, L3].)
P0117 | ECT sensor circuit low input | ON | 1 | Engine cooling system | C, O, R | × | (See DTC P0117 [L8, LF, L3].)
P0118 | ECT sensor circuit high input | ON | 1 | Engine cooling system | C, O, R | × | (See DTC P0118 [L8, LF, L3].)
P0122 | TP sensor No.1 circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0122 [L8, LF, L3].)
P0123 | TP sensor No.1 circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0123 [L8, LF, L3].)
P0125 | Excessive time to enter closed loop fuel control | ON | 2 | Engine cooling system | C | × | (See DTC P0125 [L8, LF, L3].)
P0131 | A/F sensor circuit low input | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P0131 [L8, LF, L3].)
P0132 | A/F sensor circuit high input | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P0132 [L8, LF, L3].)
P0133 | A/F sensor circuit problem | ON | 2 | A/F sensor, HO2S | C | × | (See DTC P0133 [L8, LF, L3].)
P0134 | A/F sensor no activity detected | ON | 2 | A/F sensor, HO2S | C, R | × | (See DTC P0134 [L8, LF, L3].)
P0138 | HO2S circuit high input | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P0138 [L8, LF, L3].)
P0140 | HO2S no activity detected | ON | 2 | A/F sensor, HO2S | C, R | × | (See DTC P0140 [L8, LF, L3].)
P0222 | TP sensor No.2 circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0222 [L8, LF, L3].)
P0223 | TP sensor No.2 circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0223 [L8, LF, L3].)
P0300 | Random misfire detected | Flash/ON | 1 or 2 | Misfire | C, R | × | (See DTC P0300 [L8, LF, L3].)
P0301 | Cylinder No.1 misfire detected | Flash/ON | 1 or 2 | Misfire | C, R | × | (See DTC P0301, P0302, P0303, P0304 [L8, LF, L3].)
P0302 | Cylinder No.2 misfire detected | Flash/ON | 1 or 2 | Misfire | C, R | ×
P0303 | Cylinder No.3 misfire detected | Flash/ON | 1 or 2 | Misfire | C, R | ×
P0304 | Cylinder No.4 misfire detected | Flash/ON | 1 or 2 | Misfire | C, R | ×
P0327 | KS circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P0327 [L8, LF, L3].)
P0328 | KS circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P0328 [L8, LF, L3].)
P0335 | CKP sensor circuit problem | ON | 1 | CCM | C | × | (See DTC P0335 [L8, LF, L3].)
P0340 | CMP sensor circuit problem | ON | 1 | CCM | C | × | (See DTC P0340 [L8, LF, L3].)
P0403 | EGR valve (stepper motor) circuit problem | ON | 2 | CCM | C, O, R | × | (See DTC P0403 [L8, LF, L3].)
P0420 | Warm up catalyst system efficiency below threshold | ON | 2 | Catalyst | C | × | (See DTC P0420 [L8, LF, L3].)
P0443 | Purge solenoid valve circuit problem | ON | 2 | CCM | C, O, R | × | (See DTC P0443 [L8, LF, L3].)
P0480 | Cooling fan relay No.1 control circuit malfunction | OFF | 1 | Other | C, O, R | × | (See DTC P0480 [L8, LF, L3].)
P0481*4 | Cooling fan relay No.2 and No.3 control circuit malfunction | OFF | 1 | Other | C, O, R | × | (See DTC P0481 [L3].)
P0482*3 | Cooling fan relay No.4 control circuit malfunction | OFF | 1 | Other | C, O, R | × | (See DTC P0482 [L8, LF].)
P0500 | VSS circuit problem | ON | 2 | CCM | C | × | (See DTC P0500 [L8, LF, L3].)
P0505 | IAC system problem | OFF | - | Other | R | - | (See DTC P0505 [L8, LF, L3].)
P0506 | Idle control system RPM lower than expected | ON | 2 | CCM | C | × | (See DTC P0506 [L8, LF, L3].)
P0507 | Idle control system RPM higher than expected | ON | 2 | CCM | C | × | (See DTC P0507 [L8, LF, L3].)
P0550 | PSP switch circuit malfunction | ON | 2 | Other | C | × | (See DTC P0550 [L8, LF, L3].)
P0564 | Cruise control switch circuit malfunction | OFF | 1 | Other | C | × | (See DTC P0564 [L8, LF, L3].)
P0571 | Brake switch circuit problem | OFF | 1 | Other | C | × | (See DTC P0571 [L8, LF, L3].)
P0601 | PCM memory check sum error | ON | 1 | CCM | C, O, R | × | (See DTC P0601 [L8, LF, L3].)
P0602 | PCM programming error | ON | 1 | CCM | C, O, R | × | (See DTC P0602 [L8, LF, L3].)
P0604 | PCM RAM error | ON | 1 | CCM | C, O, R | × | (See DTC P0604 [L8, LF, L3].)
P0606 | ECM/PCM processor | ON | 1 | CCM | C, O, R | × | (See DTC P0606 [L8, LF, L3].)
P0607 | PCM performance problem | OFF | 1 | Other | C, O, R | × | (See DTC P0602 [L8, LF, L3].)
P0610 | PCM vehicle options error | ON | 1 | CCM | C, O, R | × | (See DTC P0610 [L8, LF, L3].)
P0638 | Throttle actuator control circuit range/performance problem | ON | 1 | CCM | C | × | (See DTC P0638 [L8, LF, L3].)
P0661*2 | Variable intake-air solenoid valve circuit low input | OFF | 1 | Other | C, O, R | × | (See DTC P0661 [LF, L3].)
P0662*2 | Variable intake-air solenoid valve circuit high input | OFF | 1 | Other | C, O, R | × | (See DTC P0662 [LF, L3].)
P0703 | Brake switch input circuit problem | ON | 2 | CCM | C | × | (See DTC P0703 [L8, LF, L3].)
P0704*5 | Clutch pedal position (CPP) switch input circuit problem | ON | 2 | CCM | C | × | (See DTC P0704 [L8, LF, L3].)
P0850*5 | Neutral switch input circuit problem | ON | 2 | CCM | C | × | (See DTC P0850 [L8, LF, L3].)
P2009 | Variable tumble solenoid valve circuit low input | ON | 2 | CCM | C, O, R | × | (See DTC P2009 [L8, LF, L3].)
P2010 | Variable tumble solenoid valve circuit high input | ON | 2 | CCM | C, O, R | × | (See DTC P2010 [L8, LF, L3].)
P2088 | Oil control valve (OCV) circuit low | ON | 1 | CCM | C, O, R | × | (See DTC P2088 [L8, LF, L3].)
P2089 | Oil control valve (OCV) circuit high | ON | 1 | CCM | C, O, R | × | (See DTC P2089 [L8, LF, L3].)
P2096 | Target A/F feedback system too lean | ON | 2 | Fuel system | C | × | (See DTC P2096 [L8, LF, L3].)
P2097 | Target A/F feedback system too rich | ON | 2 | Fuel system | C | × | (See DTC P2097 [L8, LF, L3].)
P2100 | Throttle actuator circuit open | ON | 1 | CCM | C, O, R | × | (See DTC P2100 [L8, LF, L3].)
P2101 | Throttle actuator circuit range/performance | ON | 1 | CCM | C, R | × | (See DTC P2101 [L8, LF, L3].)
P2102 | Throttle actuator circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P2102 [L8, LF, L3].)
P2103 | Throttle actuator circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P2103 [L8, LF, L3].)
P2107 | Throttle actuator control module processor error | ON | 1 | CCM | C, R | × | (See DTC P2107 [L8, LF, L3].)
P2108 | Throttle actuator control module performance error | ON | 1 | CCM | C, R | × | (See DTC P2108 [L8, LF, L3].)
P2119 | Throttle actuator control throttle body range/performance problem | ON | 1 | CCM | C, R | × | (See DTC P2119 [L8, LF, L3].)
P2122 | APP sensor No.1 circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P2122 [L8, LF, L3].)
P2123 | APP sensor No.1 circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P2123 [L8, LF, L3].)
P2127 | APP sensor No.2 circuit low input | ON | 1 | CCM | C, O, R | × | (See DTC P2127 [L8, LF, L3].)
P2128 | APP sensor No.2 circuit high input | ON | 1 | CCM | C, O, R | × | (See DTC P2128 [L8, LF, L3].)
P2135 | TP sensor No.1/No.2 voltage correlation problem | ON | 1 | CCM | C, O, R | × | (See DTC P2135 [L8, LF, L3].)
P2138 | APP sensor No.1/No.2 voltage correlation problem | ON | 1 | CCM | C, O, R | × | (See DTC P2138 [L8, LF, L3].)
P2177 | Fuel system too lean at off idle | ON | 2 | Fuel system | C, R | × | (See DTC P2177 [L8, LF, L3].)
P2178 | Fuel system too rich at off idle | ON | 2 | Fuel system | C, R | × | (See DTC P2178 [L8, LF, L3].)
P2187 | Fuel system too lean at idle | ON | 2 | Fuel system | C, R | × | (See DTC P2187 [L8, LF, L3].)
P2188 | Fuel system too rich at idle | ON | 2 | Fuel system | C, R | × | (See DTC P2188 [L8, LF, L3].)
P2195 | A/F sensor signal stuck lean | ON | 2 | A/F sensor, HO2S | C | × | (See DTC P2195 [L8, LF, L3].)
P2196 | A/F sensor signal stuck rich | ON | 2 | A/F sensor, HO2S | C | × | (See DTC P2196 [L8, LF, L3].)
P2237 | A/F sensor positive current control circuit open | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P2237 [L8, LF, L3].)
P2251 | A/F sensor negative current control circuit open | ON | 2 | A/F sensor, HO2S | C, O, R | × | (See DTC P2251 [L8, LF, L3].)
P2502 | Charging system voltage problem | OFF | 1 | Other | C, R | × | (See DTC P2502 [L8, LF, L3].)
P2503 | Charging system voltage low | OFF | 1 | Other | C, R | × | (See DTC P2503 [L8, LF, L3].)
P2504 | Charging system voltage high | OFF | 1 | Other | C, R | × | (See DTC P2504 [L8, LF, L3].)
P2507 | PCM B+ voltage low | ON | 1 | CCM | C, O, R | × | (See DTC P2507 [L8, LF, L3].)
P2676*4 | Variable air duct (VAD) solenoid valve circuit low input | OFF | 1 | Other | C, O, R | × | (See DTC P2676 [L3].)
P2677*4 | Variable air duct (VAD) solenoid valve circuit high input | OFF | 1 | Other | C, O, R | × | (See DTC P2677 [L3].)
U0073 | CAN system communication error | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0101*6 | Communication error to TCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0121 | Communication error to ABS HU/CM or DSC HU/CM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0155 | Communication error to instrument cluster | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])

  *1 :
C: CMDTC self-test, O: KOEO self-test, R: KOER self-test
  *2 :
LF, L3
  *3 :
L8, LF
  *4 :
L3
  *5 :
MTX
  *6 :
ATX