#
REAR COMBINATION LIGHT REMOVAL/INSTALLATION

id091800465500

1. Disconnect the negative battery cable.

2. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION [4SD, 5HB].) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION [WGN].)

3. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Rear combination light
4 | Socket
5 | Rear turn light bulb
6 | Brake light/taillight bulb

4. Install in the reverse order of removal.