#
NO.11 SHIFT POINT IS HIGH OR LOW [JA5AX-EL]

id050305801600

11 | Shift point is high or low
DESCRIPTION | • Shift point considerably different from automatic shift diagram. • Shift delays when accelerating. • Shift occurs quickly when accelerating and engine speed does not increase.
POSSIBLE CAUSE | • If the transaxle does not shift abnormally, there is a malfunction of input signal to TP sensor, input/turbine speed sensor, or VSS. • If engine speed is high or low regardless that shifting is normal, inspect tachometer. • Verify that output signal of TP sensor changes linearly. Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.