#
BCM SELF-TEST

id0902j0830600

1. Connect the WDS or equivalent to the DLC-2.

2. Set up the WDS or equivalent (including the vehicle recognition).

3. Verify the following vehicle conditions:

  • Ignition switch is at ON position.
  • All the switches are turned off (except the ignition switch).
  • All the doors, bonnet, trunk lid, and liftgate are closed.
  • All the doors, and liftgate are unlocked.
  • Parking brake lever is pulled.
  • Hazard warning switch is turned to off.
  • Turn switch is turned to off.
  • Rear wiper switch is turned to off.

4. Perform procedures according to directions on the WDS or equivalent screen.

5. Verify if any DTCs are displayed.

  • If any DTCs are displayed, perform the troubleshooting according to the corresponding DTC inspection.

6. Disconnect the WDS or equivalent.