#
EGR COOLER REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0116f1099000

1. Disconnect the negative battery cable.

2. Remove the engine cover.

3. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

4. Remove the air cleaner and air inlet hose. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

5. Remove the battery. (See BATTERY REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

6. Remove the air inlet pipe and turbocharger air outlet pipe. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

7. Remove in the order indicated in the table.

1 | Water hose
2 | EGR cooler

8. Install in the reverse order of removal.