#
ENGINE DISASSEMBLY/ASSEMBLY [L3 Turbo]

id0110b3800500

1. Remove the engine from the transaxle. (See MANUAL TRANSAXLE REMOVAL/INSTALLATION [A26MX-R].)

2. Remove the intake-air system. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

3. Remove the exhaust system. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

4. Remove the generator. (See GENERATOR REMOVAL/INSTALLATION [L3 Turbo].)

5. Remove the starter. (See STARTER REMOVAL/INSTALLATION [L3 Turbo].)

6. Remove the CKP sensor. (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [L3 Turbo].)

7. Install in the reverse order of removal.