#
EGR VALVE REMOVAL/INSTALLATION [L3 Turbo]

id0116b4801000

1. Disconnect the negative battery cable.

2. Disconnect the EGR valve connector.

3. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT [L8, LF, L3, L3 Turbo].)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

1 | Water hose
2 | EGR valve (See EGR Valve Removal Note.)

## EGR Valve Removal Note

1. Remove the air hose. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)