#
CENTER PILLAR INSTALLATION

D6E098070350B02

1. When joining and cutting the new and existing parts, trial fit the new part in position, then measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for plug welds before installing new parts.

  Note

  • In areas where the outer, reinforcement, inner, etc. are in 3-4 layers, drill holes for plug welds in all but the innermost panel.

  Warning

  • When cutting and joining the reinforcement, make sure not to damage or scratch the B-pillar reinforcement.

3. Install in the following order: inner, reinforcement, and outer.

4. After temporarily installing new parts, make sure the related parts fit properly.