#
TRUNK SIDE TRIM REMOVAL/INSTALLATION [4SD, 5HB]

id0917004623a1

## 4SD

1. Remove the trunk end trim.

2. Remove the fasteners, then remove the trunk side trim.

3. Install in the reverse order of removal.

## 5HB

1. Remove the trunk end trim.

2. Remove the trunk side upper trim.

3. Remove the cargo hooks.

4. Remove the fasteners.

5. Pull the trunk side trim toward you, then disengage clips A from the body.

6. Install in the reverse order of removal.