#
LIFTGATE ADJUSTMENT [5HB]

id091100800901

1. Measure the gap and height between the liftgate and the body.

2. If there is any malfunction, loosen the liftgate hinge installation bolts or the liftgate striker installation screws, and reposition the liftgate.

Clearance

  a: 3.0-7.0 mm {0.12-0.28 in}
  b: -1.0-3.4 mm {-0.04-013 in}
  c: 2.8-5.2 mm {0.11-0.24 in}
  d: -1.2-1.2 mm {0.05-0.05 in}
  e: 2.8-5.8 mm {0.11-0.22 in}
  f:4.0-8.0 mm {0.16-0.31 in}

3. Tighten the bolts or screws.